U-Boot SPL 2013.10-g0451b05 (Jun 16 2017 - 11:39:04)
MitySOM335x profile 1 - Model No: 3352-HX-X4A-RC Serial No: 15013530
Critical Link: Error u-boot not compiled with for 1GB nand support. Nand may not function correctly.
Configuring for 1024 MB DDR3 @ 400MHz
Critical Link AM335X Dev Kit -- NAND Page size = 2048k booting from dev 8
reading u-boot.img
reading u-boot.img


U-Boot 2013.10-g0451b05 (Jun 16 2017 - 11:39:04)

AM335X-GP rev 2
I2C:   ready
DRAM:  1 GiB
WARNING: Caches not enabled
Critical Link: Error u-boot not compiled with for 1GB nand support. Nand may not function correctly.
NAND:  Using 2k bch8 layout
ECC Mode = 2 lo = 56/0
1024 MiB
MMC:   OMAP SD/MMC: 0, OMAP SD/MMC: 1
*** Warning - bad CRC, using default environment

Net:   cpsw:1 is connected to cpsw.  Reconnecting to cpsw
cpsw, usb_ether
Hit any key to stop autoboot:  0
U-Boot# setenv fdtaddr 0x88000000; setenv fdt_high 0xFFFFFFFF
U-Boot# setenv serverip 10.0.102.252
U-Boot# dhcp; tftp $fdtaddr am335x-mitysom.dtb; tftp $kloadaddr zImage; bootz $kloadaddr - $fdtaddr
link up on port 0, speed 1000, full duplex
link up on port 1, speed 1000, full duplex
BOOTP broadcast 1
DHCP client bound to address 10.0.102.156
Using cpsw device
TFTP from server 10.0.102.252; our IP address is 10.0.102.156
Filename 'uImage'.
Load address: 0x82000000
Loading: #################################################################
         #################################################################
         #################################################################
         ########################################
         1.4 MiB/s
done
Bytes transferred = 3447288 (3499f8 hex)
link up on port 0, speed 1000, full duplex
link up on port 1, speed 1000, full duplex
Using cpsw device
TFTP from server 10.0.102.252; our IP address is 10.0.102.156
Filename 'am335x-mitysom.dtb'.
Load address: 0x88000000
Loading: ###
         1.2 MiB/s
done
Bytes transferred = 37210 (915a hex)
link up on port 0, speed 1000, full duplex
link up on port 1, speed 1000, full duplex
Using cpsw device
TFTP from server 10.0.102.252; our IP address is 10.0.102.156
Filename 'zImage'.
Load address: 0x80007fc0
Loading: #################################################################
         #################################################################
         #################################################################
         ################################################
         1.4 MiB/s
done
Bytes transferred = 3560808 (365568 hex)
Kernel image @ 0x80007fc0 [ 0x000000 - 0x365568 ]
## Flattened Device Tree blob at 88000000
   Booting using the fdt blob at 0x88000000
   Using Device Tree in place at 88000000, end 8800c159

Starting kernel ...



,--.   ,--.,--.  ,--.            ,---.   ,-----. ,--.   ,--.
|   `.'   |`--',-'  '-.,--. ,--.'   .-' '  .-.  '|   `.'   |
|  |'.'|  |,--.'-.  .-' \  '  / `.  `-. |  | |  ||  |'.'|  |
|  |   |  ||  |  |  |    \   '  .-'    |'  '-'  '|  |   |  |
`--'   `--'`--'  `--'  .-'  /   `-----'  `-----' `--'   `--'
                       `---'
              ,----. ,----. ,-----.,--.   ,--.
              '.-.  |'.-.  ||  .--' \  `.'  /
                .' <   .' < '--. `\  .'    \
              /'-'  |/'-'  |.--'  / /  .'.  \
              `----' `----' `----' '--'   '--'

Critical Link LLC http://support.criticallink.com mitysom-335x /dev/ttyO0
        Linux kernel verison Linux armv7l #1 Mon Jun 19 11:50:02 EDT 2017

Critical Link Linux (sysvinit) 1.6.0 mitysom-335x /dev/ttyO0

mitysom-335x login: root
root@mitysom-335x:~#
